

The camera menu (pictured below) is not available in the CMS client because it is added using ONVIF or other protocols and must be added with the male-Mai protocol (H264DVR) to pull the camera menu



Disconnect the camera connection. (The camera is disconnected before it can be modified, double-click the camera IP to disconnect), and then modify the following procedure.

